Arduino 2 borden

Onderdelen

2x LED lampjes

2x resitor

4 kabels (jump wires)

2x arduino UNO

const int LED = 3;

void setup() {

// put your setup code here, to run once:

pinMode (LED, OUTPUT);

}

void loop() {

// put your main code here, to run repeatedly:

digitalWrite (LED,HIGH);

delay (1000);

digitalWrite (LED, LOW);

delay (1000);

}

